PLANET 48-Port ADSL 2/2+ IP DSLAM Firmware Release
--------------------------------------------------

Device Supported:       IDL-4802 / IDL-4802-48
Release Date:           05/05/2009
New Release Version:    0.79B02
Previous Release:       Initial Release



Added Features and Firmware Changes:
====================================
Version 0.79B02 
1. Initial release version



Firmware Upgrade Procedure:
===========================
If you want to update the firmware, you must get the firmware image file from FTP Server.
Suppose that FTP Server IP address is 210.66.155.77 and the image filename is "FW-IDL4802_101B02". 

To perform the firmware upgrade:
Step 1.  Put the firmware files(FW-IDL4802_079B02 and FW-IDL4802_079B02sum) on your 
         default direction of FTP server. These two files must put in the same folder. 

Step 2.  Login IDL-4802 via Console (9600, 8, n, 1, n).
         login:admin
         password:admin

Step 3.  Command: "enable" --> Go to enable mode.
         
Step 4.  Command: "configure" --> Go to configuration mode.

Step 5.  Command: "firmware login 210.66.155.77 username test password test"

Step 6.  Command: "firmware upgrade FW-IDL4802_079B02"

Firmware upgrade may take a few minutes, don't turn off or reset the system during the process. 
You can get status using command "show firmware status" in Enable execution mode.

         exit --> back to enable mode
         show firmware status

When status returns "Upgraded already!", you can restart the system to run new firmware image.
Once you upgrade successfully, you can't upgrade the second time unless you have restarted the system.

Step 7.  Command: "system restart" --> Restart the IDL-4802.


Note: 
Do not turn the power off during the upgrade process. This will damage the unit.


Thanks for choosing PLANET products, any comment or feedback will be appreciated.


Best Regards ,

PLANET Tech Support Team

Technical support:support@planet.com.tw