PLANET 48-Port ADSL 2/2+ IP DSLAM Firmware Release
--------------------------------------------------

Device Supported:       IDL-4802 / IDL-4802-48
Release Date:           07/12/2011
New Release Version:    0.86PN_B01
Previous Release:       0.85PN_B01

Added Features and Firmware Changes:
====================================
1. Remove first login and password expiry.
2. SNMP community name change issue. 
   (1) while modifying snmp community, it would delete it and then re-create it. Yet the 1st community can't delete
   (2) snmp community accept special symbols (` ~ ! @ # $ % ^ & * ( ) - _ + = [ ] { } : ; , .) except space and "\" and "?"
3. Fix ATM cell byte counter double issue. 
   (1)ATM statistics counter. 
   (2)ATM cell RX byte counter always double count.
4. Fix while system working in "snooping mode" after system reboot then the IGMP query from uplink server can not pass.
5. Fix the change command line's prompt (hostname) and save issue.
 (When change hostname, the prompt in CLI should change run time for current session, and next login should change.)

Previous Release History:
=========================
Version 0.85PN_B01
1.Fix Syslog process is activated when system is reboot, even the syslog is disabled with UI.
2.Fix the supported length for 'path+image name' for remote download is only 31-byte. It is usually inadequate for operation.
3.Fix after reboot system , NoiseMargin 4 parameters become 10 times of saved value.
4.Fix Ethernet Statistic:No input unknown protocol packets field at WEB-GUI
5.Fix IDL-4802 will not reject illegal SNRM settings for SRA function which will result in DSL chipset work abnormally
6.Fix 802.1x Web GUI has indisposed text on the pages.
7.Fix upstream PBO
8.Fix the DownShift of the DS/US must smaller than UpShift of the DS/US in ADSL Service Channel Profile.
9.Fix system can't response ARP package

Previous Release History:
=========================
Version 0.79B02 
1. Initial release version



Firmware Upgrade Procedure:
===========================
If you want to update the firmware, you must get the firmware image file from FTP Server.
Suppose that FTP Server IP address is 210.66.155.77 and the image filename is "FW-IDL4802_101B02". 

To perform the firmware upgrade:
Step 1.  Put the firmware files(FW-IDL4802_079B02 and FW-IDL4802_079B02sum) on your 
         default direction of FTP server. These two files must put in the same folder. 

Step 2.  Login IDL-4802 via Console (9600, 8, n, 1, n).
         login:admin
         password:admin

Step 3.  Command: "enable" --> Go to enable mode.
         
Step 4.  Command: "configure" --> Go to configuration mode.

Step 5.  Command: "firmware login 210.66.155.77 username test password test"

Step 6.  Command: "firmware upgrade FW-IDL4802_079B02"

Firmware upgrade may take a few minutes, don't turn off or reset the system during the process. 
You can get status using command "show firmware status" in Enable execution mode.

         exit --> back to enable mode
         show firmware status

When status returns "Upgraded already!", you can restart the system to run new firmware image.
Once you upgrade successfully, you can't upgrade the second time unless you have restarted the system.

Step 7.  Command: "system restart" --> Restart the IDL-4802.


Note: 
Do not turn the power off during the upgrade process. This will damage the unit.


Thanks for choosing PLANET products, any comment or feedback will be appreciated.


Best Regards ,

PLANET Tech Support Team

Technical support:support@planet.com.tw