Thanks for purchasing PLANET IGS-20040MT Layer 2+ Industrial 16-Port 10/100/1000T + 4-Port 100/1000X SFP Managed Switch.
This document provides the firmware release note and history of the products below:

Version 1.342c150127 Released on 2/2/2015
=======================================
Firmware version: v1.342c150127
Hardware version: 1.0
File Name: FW-IGS-20040MT_V1.342c150127.dat
File Size: 4,760,527 bytes 
Release Date: 2/2/2015
=======================================
Function enhanced

This firmware provides the following modifications:

A: Bug Fixed -
    (1) Fixed the hardware reset button that could not function properly at times.   
   
B. Function Added -
    NA

C. Other:
    NA

D. Known Issue:
    NA.



[Upgrade Requirements]:

1. The latest firmware version of IGS-20040MT
2. The IGS-20040MT Industrial Switch
3. Workstation with Microsoft IE 7.0 or above.
4. TFTP server.


[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target Switch.

2. Login is required to access the Web interface after the Switch boot completes successfully. The factory default user name and password are "admin".

3. After the Web main screen appears, click the "System"\"TFTP Firmware Upgrade" on the left side of the menu.  

4. The screen will be directed to the "TFTP Firmware Upgrade" page. Enter values as shown below.
   a. Enter the TFTP IP address.
   b. Firmware File Name: Please enter firmware file name, like "FW-IGS-20040MT_V1.340b141023.dat"

5. Click the "Upgrade" button to start the firmware upgrade procedure. 

6. When the confirm message pops up, click "OK". The Switch will start the TFTP upgrade procedure.

7. Please don't power off the Switch while the procedure is underway.

8. Please check your TFTP server application to confirm whether the TFTP file is well transmitted to the Switch.

9. The Switch will reboot then, and it will take 2 to 3 minutes for the TFTP firmware to upgrade and reboot the procedure. 
   Please wait for the process to complete.

10. Once the new software is loaded to the system successfully, the login screen appears. 

11. Enter the user name and password to login the Switch.

12. Relogin the Switch via Web browser. Please click the "System \ "System Information" to double-check if the firmware is upgraded successfully.

 

*********************************
Firmware Release History:  
*********************************

Version 1.340b141023 Released at 2014/11/05
=======================================
Firmware version: v1.340b141023
Hardware version: 1.0
File Name: FW-IGS-20040MT_V1.340b141023.dat
File Size: 4,724,447 bytes 
Release at 2014/11/5
=======================================
Function enhance

This firmware provides the following modification:

A: Bug Fixed -
    (1) Fixed the console will show auto 1000 words repeatly   

=======================================
Version 1.340b140924 Released at 2014/9/24
=======================================
Firmware version: v1.340b140217
Hardware version: 1.0
File Name: FW-IGS-20040MT_1.340b140924.dat
Release at 2014/9/24
=======================================

Initial Release

Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw


